|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Serial No. | Remark | Description | Quantity | Unit | Rate | Amount |
| E-01 |  | Minimum lumen output 2500 Im Post top Luminarie | 2.0 | Each | 5075.0 | 10150 |
| E-02 |  | 6 A 3/5 pin shuttered socket | 4.0 | Each | 107.0 | 428 |
| E-03 |  | 6/16 A shuttered socket | 5.0 | Each | 176.0 | 880 |
| E-04 |  | Providing & Fixing of modular type lockable feature socket duly made out of unbreakable and fire retardant vergin poly carbonate with brass terminals and captive screws & silver alloy contact tip with IP-20 rating, including all as per pre approved by Engineer in charge, making connections, testing etc. as required. For additional technical parameters of product / work refer Annexure 'A' attached with this BSR | 5.0 | Each | 345.0 | 1725 |
| E-05 |  | 6 A 3/5 pin shuttered socket | 4.0 | Each | 107.0 | 428 |
| E-06 |  | 6/16 A shuttered socket | 5.0 | Each | 176.0 | 880 |